STATUS: Finished / In-Progress

GameCube Mods and Repair

modding and repair of GameCube systems.

Items Needed

Xeno ModChip

Laser assembly

Instructions

Step 1

Step 2

NOTES

Laser Eye Assembly always needs tweaked. LOWER Ohms = MORE LASER

Start with higher resistance and work your way down slowly.

200 to 500 Ohms is the average resistance. DO NOT GO UNDER 175!!!

001 GC laser needs resistance set between 450 - 600 101 GC laser needs resistance set between 150 - 250

More Information

A youtube or URL etc