STATUS: Finished / In-Progress

GameCube Mods and Repair

modding and repair of GameCube systems.

Items Needed

Xeno ModChip

Laser assembly

Instructions

Step 1

Step 2

NOTES

Laser Eye Assembly always needs the potentiometer tweaked. Measure the resistance across the left leg and bottom right leg

LOWER Ohms = MORE LASER

Start with higher resistance and work your way down slowly.

200 to 500 Ohms is the average resistance. DO NOT GO UNDER 175!!!

001 GC laser needs resistance set between 450 - 600

101 GC laser needs resistance set between 150 - 250

Examples: Jon's old GC started at 216 and read at 196; Marc's newer GC started at 276 and read at 199

More Information

A youtube or URL etc